VERSA-VENT SELF INSTALL KIT (INCLUDES 2 VENTS)

SEIZMIK PART #: 90049

FITMENT INFO: For Polycarbonate Windshields Only

WARNING: Installation requires cutting your windshield.  Please read directions carefully and install AT YOUR OWN RISK.  Only attempt to cut polycarbonate windshields. Acrylic windshields will most likely crack if you attempt to install this kit. DO NOT attempt to install in glass.

The Versa-Vent self install kit from Seizmik, includes 2 Seizmik Versa-Vents, cutting template, and all mounting hardware. The dual vent system is designed to add driver and passenger ventilation and anti-fogging features to polycarbonate windshields. The Versa-Vent features a defog mode. The vent is made of glass filled nylon, so it’s incredibly durable. The scoop on the front gathers up air off the hood and re-directs it to inside the vehicle so even at very slow speeds there is a surprising amount of air that can come through the vent. The design of the scoop and the gasket between it and the windshield keeps precipitation out while still allowing airflow in—as much or as little as either the driver or passenger desires.

The innovative windshield vents include the following features:

•	Made of super-durable glass-filled nylon
•	Designed with built-in defogging vents
•	Gasket sealed against water intrusion
•	Fully adjustable easy-to-use louver for variable airflow